TSPi Inspection Report: Form INS

	Name
	Publisher code module
	Date
	02/07/2002

	Team
	Dragon
	Instructor
	Dr. W. Honig

	Part/Level
	Part
	Cycle
	     1

	Moderator
	Xiaoyu
	
	Owner
	Lilin 

	
	

	Engineer Data
	

	Name
	Defects
 
	Preparation Data
	Est.

	
	Major
	Minor
	Size

(LOC)
	Time (min)


	Rate 

(Loc /hour)
	Yield

(major defects only)

	Kyle          (K) ( (A)
	3
	2
	125
	60
	125
	33%

	Michael    (M)
	3
	1
	125
	120
	62.5
	33%

	LuCai        (L) 
	2
	1
	125
	90
	83.3
	22%

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	Totals:
	8
	4
	375
	270 min = 4.5 hr
	83.3 (avg)
	5/9 = 56%

	

	Defect Data
	

	No.
	Defect Description
	Defects 
	Engineers (finding major defects)

	
	
	Maj
	Min
	K
	M
	L
	
	A
	B

	1
	Various typographical errors (e.g., punctuation, capitalization, etc.)
	
	2
	1
	2
	2
	
	
	

	2
	Author error checks are missing, line 8-9
	1
	
	1u
	
	
	
	1u
	

	3
	Not following style, line 10-15
	
	1
	
	1
	1
	
	
	

	4
	Publisher name incorrectly sent to screen, line 25
	1
	
	1
	1
	1
	
	1
	1

	5
	Loop runs once too many times, line 29-54
	1
	
	1u
	
	
	
	1u
	

	6
	Wrong data base access, line 34
	1
	
	
	1u
	
	
	
	1u

	7
	Need comments to clarify function, line 112
	
	1
	1
	
	
	
	
	

	8
	Author code needed, not name, line 120
	1
	
	
	1
	1
	
	
	1u

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	

	Totals
	5
	4
	3
	3
	2
	
	3
	3

	Unique Defects
	
	2
	1
	0
	
	2
	2

	
	

	Inspection Summary
	
	Product Size:
	125 
	Size Measure:
	Loc

	Total defects for A:
	3
	Total defects for B:
	3
	C (# common):
	1

	Total Defects (AB/C):
	9
	Number Found (A+B-C):
	5
	Number Left:
	4

	Meeting Time: (hours)
	1 
	Total Inspection Hours:
	9.5
	Overall Rate: (loc/hour)
	13.2


Note:  Accuracy improves when total major defects > 4 and common defects found >= 2. If common defect = 0 enter inf  for an infinite number left.  Round Total Defects and Number Left to the nearest whole number.
u used to mark unique major defects

Estimated Yield in Engineer Data is calculated at the END of the inspection based on total major defect left (as predicted in Number Left).  If Number Left is inf, enter 0.

Version 3.0 (25 Sept 08)

Updating time to minutes and minor error updates
1 Major defects either change the program source code or would ultimately cause a source code change if not fixed in time; all other defects are considered minor.





